## Truck Mounted Attenuator (TMA) National Register

Followingan approach to suppliers for detail on the required truck weight, NZTA has established the following minimum truck weights:

|  |  |  |
| --- | --- | --- |
| Manufacturer / Supplier | TMA System | Minimum Truck Weight |
| **Barrier Systems Inc** | UMAD-70k | 6400 kg (- 400 kg) |
| **Energy Absorption Systems Inc** | Alpha-70k | 6400 kg (- 400 kg) |
| **Traffix Devices Inc** | Scorpion 10,000 | 6400 kg (- 400 kg) |

NB: The UMAD was 9000kg it has been retested and is now cleared for 6400